



**Compliance of the offer**

**- Version N°01**

**Document No 227.185**

**NOT FOR OFFICIAL USE**

**COURTESY TRANSLATION, THE FRENCH VERSION IS THE REFERENCE FOR THE CONTRACT**

# Administrative Compliance

| **Administrative compliance** | **Commission validation** |
| --- | --- |
| **Wording** | **Compliance (YES/NO)** | **If applicable, justification document** |
| Eligibility | Not in a state of bankruptcy, liquidation, judicial settlement, cessation of activity, or in any analogous situation resulting from a procedure of the same nature existing in national laws and regulations |  |  |  |
| Is not the subject of a procedure of declaration of bankruptcy, liquidation, legal settlement or any other procedure of the same nature existing in national laws and regulations |  |  |  |
| Is not the subject of a conviction pronounced by a judgment having the force of res judicata (that is to say, against which there is no longer any possible appeal) for any offense involving their professional conduct |  |  |  |
| In professional matters, has not committed serious misconduct |  |  |  |
| Has fulfilled its obligations relating to the payment of social security contributions according to the legal provisions of the country where the company is established |  |  |  |
| Has fulfilled its obligations relating to the payment of taxes and duties according to the legal provisions of the country where the company is established |  |  |  |
| Has not been seriously guilty of misrepresentation in providing the information required by DCI for its participation in a contract |  |  |  |
| Does not act as a front company created to conceal financial transactions and/or launder money from one or more other companies |  |  |  |
| In the context of another contract entered into with DCI, has not been declared in serious breach of performance due to non-compliance with its contractual obligations |  |  |  |
| It has not been established by a final judgment that the company is guilty of any of the following facts:i. fraud, within the meaning of Article 3 of Directive (EU) 2017/1371;ii. corruption, as defined in Article 4(2) of Directive (EU) 2071/1371;iii. behavior linked to a criminal organization referred to in Article 2 of the Framework Decisioniv. 2008/841/JHA of the Council;v. money laundering or terrorist financing within the meaning of Article 1, paragraphs 3, 4 and 5 of Directive (EU) 2015/849 of the European Parliament and of the Council;vi. terrorist offense or offense related to terrorist activities, as defined respectively in Article 1 and Article 3 of Council Framework Decision 2002/475/JHA, or incitement to commit an offence, complicity or attempt infringement as referred to in Article 4 of the said decision;vii. child labor or other forms of trafficking in human beings as defined in Article 2 of Directive 2011/36/EU of the European Parliament and of the Council; |  |  |  |
| Benefit does not exceed 50% of turnover |  |  |  |
| Professional experience of at least 5 years in the same field as the call for tenders |  |  |  |
| Performing a service of the same type |  |  |  |
| Documents | Declaration of honor signed |  |  |  |
| Document justifying registration as a legal person |  |  |  |
| Vigilance certificate |  |  |  |
| civil liability certificate |  |  |  |
| description of the product warranty organization |  |  |  |
| The certificate of vigilance issued by the collection agency to which it belong, which states that the company is up to date with all of its social obligations |  |  |  |
| Form | Deadline for submitting the offer respected |  |  |  |
| Complete offer |  |  |  |
| Offer in French or with an English translation |  |  |  |
| Period of validity of offers |  |  |  |

# Compliance with technical requirements

| **Technical specification's DCI Binoculars** | **Technical offer VHF transceiver** | **Validation committee** |
| --- | --- | --- |
| **Reference** | **Contractual requirement** | **Compliant (C) / Non- Compliant (NC)** | **Compliance justification in the offer (page, chapter , paragraph , etc.)** |
| **EX-1** | Marine VHF radio |  |  |  |
| **EX-2** | Fixed mount type |  |  |  |
| **EX-3** | Transmitter out power : 25W (high), 1 W (low) |  |  |  |
| **EX-4** | TX frequency range : 156,025MHz to 161,600 MHz |  |  |  |
| **EX-5** | RX frequency range : 156,050MHz to 163,275 MHz |  |  |  |
| **EX-6** | Wide angle colour TFT LCD (day and night modes) |  |  |  |
| **EX-7** | Digital Selective Calling (DSC) |  |  |  |
| **EX-8** | Plotter, Target list and Danger list can be toggled on the display |  |  |  |
| **EX-9** | Active noise cancelling |  |  |  |
| **EX-10** | Man Overboard Operation |  |  |  |
| **EX-11** | NMEA 2000™, NMEA 0183 connectivity |  |  |  |
| **EX-12** | IP67 Protection |  |  |  |
| **EX-13** | Compatible with 12 V / 24V power sources, power cable supplied |  |  |  |
| **EX-15** | Operating temperature: -20°C to 55°C |  |  |  |
| **EX-16** | Speaker microphone supplied |  |  |  |
| **EX-17** | Antenna, tripod for antenna and antenna cable supplied |  |  |  |
| **EX-18** | Mount kit supplied |  |  |  |
| **EX-19** | Warranty : ≥ 2 years |  |  |  |
| **EX-20** | The 100 VHF radio must have an identical configuration |  |  |  |
| **EX-21** | Each VHF radio is delivered with its user manual in English  |  |  |  |
| **EX-22** | The VHF radio packaging is compliant with international standards and they protects the radios against the shocks, high temperature and humidity. The packaging are sealed during shipping. |  |  |  |
| **EX-23** | The 100 VHF transceivers are delivered before 3 months after order |  |  |  |

| **Technical specification's DCI Telescopes** | **Technical offer AIS receiver transponder** | **Validation committee** |
| --- | --- | --- |
| **Reference** | **Contractual requirement** | **Compliant (C) / Non- Compliant (NC)** | **Compliance justification in the offer (page, chapter , paragraph , etc.)** |
| **EX-1** | AIS Class A SOLAS |  |  |  |
| **EX-2** | The AIS is a Emitter, Receiver and transponder equipment |  |  |  |
| **EX-3** | The AIS has a wide angle colour TFT LCD (day and night modes) |  |  |  |
| **EX-4** | Simplified Navigation Function |  |  |  |
| **EX-5** | Navigation to Man Over Board (MOB) Waypoint |  |  |  |
| **EX-6** | Collision alarm function |  |  |  |
| **EX-7** | Anchor watch function with audible alarm |  |  |  |
| **EX-8** | AIS target list vessels and details |  |  |  |
| **EX-9** | Closest Point of Approach (CPA) |  |  |  |
| **EX-10** | Silent mode for security and privacy |  |  |  |
| **EX-11** | Time to Closest Point of Approach (TCPA) |  |  |  |
| **EX-12** | Individual DSC call with connected marine VHF |  |  |  |
| **EX-13** | Supplied with GNSS antenna and receiver |  |  |  |
| **EX-14** | NMEA 2000™, NMEA 0183 connectivity |  |  |  |
| **EX-15** | Plug and play |  |  |  |
| **EX-16** | IP67 Protection |  |  |  |
| **EX-17** | Compatible with both 12 V and 24 V power sources |  |  |  |
| **EX-18** | DC power cable and mounting bracket kit |  |  |  |
| **EX-19** | VHF antenna, tripod and cable with length greater than 3 m |  |  |  |
| **EX-20** | Max Weight 2Kg |  |  |  |
| **EX-21** | Each AIS emitter receiver is delivered with its user manual in English |  |  |  |
| **EX-22** | Warranty : ≥ 1 years |  |  |  |
| **EX-23** | The 50 AIS emitter receiver must have an identical configuration |  |  |  |
| **EX-24** | The AIS emitter receiver packaging is compliant with international standards and they protects the receivers against the shocks, high temperature and humidity. The packaging are sealed during shipping. |  |  |  |
| **EX-25** | Individual factory control certificate supplied |  |  |  |
| **EX-26** | The 50 AIS emitter receivers are delivered before 3 months after order |  |  |  |